{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H3V1B2","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Уровень звукового давления","Hагрев","","Ном.","дБ(A)","48","48","","50","50"]
["","Охлаждение","","Ном.","дБ(A)","47","47","","48","48"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1","","1","1"]
["","Пакет для винтов","","","","1","1","","1","1"]
["","Сливная пробка","","","","1","1","","1","1"]
["Хладагент","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","ПГП","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","кг","1.20","1.20","","1.60","1.60"]
["","Тип","","","","R-410A","R-410A","","R-410A","R-410A"]
["Подсоединение труб","Перепад уровней","IU - IU","Макс.","м","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Макс.","м","15","15","","15","15"]
["","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)","","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)"]
["","Общая длина трубопроводов","Система","Фактическая","м","30","30","","30","30"]
["Compressor","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","765","765","","765","765"]
["","","","Глубина","мм","285","285","","285","285"]
["","","","Высота","мм","550","550","","550","550"]
["Масса","Блок","","","кг","38","38","","42","42"]
["Power supply","Фаза","","","","1~","1~","","1~","1~"]
["","Частота","","","Гц","50","50","","50","50"]
["","Напряжение","","","V","220-240","220-240","","220-240","220-240"]
["Примечания","","","","","(1) - Содержит фторированные парниковые газы","(1) - Содержит фторированные парниковые газы","","(1) - Содержит фторированные парниковые газы","(1) - Содержит фторированные парниковые газы"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","550","","","550"]
["","","","Ширина","мм","","","765","","","765"]
["","","","Глубина","мм","","","285","","","285"]
["Масса","Блок","","","кг","","","38","","","42"]
["Compressor","Тип","","","","","","Герметичный компрессор ротационного типа","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","","","10","","","10"]
["","","","Макс.","°CDB","","","46","","","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","","-15","","","-15"]
["","","","Макс.","°CWB","","","15.5","","","15.5"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","","","47","","","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","","","48","","","50"]
["Хладагент","Тип","","","","","","R-410A","","","R-410A"]
["","Заправка","","","кг","","","1.20","","","1.60"]
["","Заправка","","","tCO2Eq","","","2.5","","","3.3"]
["","ПГП","","","","","","2087.5","","","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","","20","","","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","","","0,02 (для длины труб свыше 20 м)","","","0,02 (для длины труб свыше 20 м)"]
["","перепад уровня","IU - OU","Макс.","м","","","15","","","15"]
["","","IU - IU","Макс.","м","","","7.5","","","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","","","30","","","30"]
["Стандартные аксессуары","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Электропитание","Фаза","","","","","","1~","","","1~"]
["","Частота","","","Гц","","","50","","","50"]
["","Напряжение","","","V","","","220-240","","","220-240"]
["Стандартные аксессуары","Узел переходника","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]