{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-F"]
[]
[]
[]
[]
["","","","","","4MXS68F3V1B2","4MXS68F3V1B","4MXS68F2V1B"]
["Уровень звукового давления","Hагрев","","Ном.","дБA","49","49"]
["","Охлаждение","","Ном.","дБA","48","48"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1"]
["","Сливная пробка","","","","1","1"]
["","Узел переходника","","","","1","1"]
["Хладагент","Charge","","","TCO2Eq","5.4","5.4"]
["","ПГП","","","","2,087.5","2,087.5"]
["","Заправка","","","кг","2.6","2.6"]
["","Тип","","","","R-410A","R-410A"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Макс.","°C сух.т.","46"]
["","","","Мин.","°C сух.т.","-10"]
["","Hагрев","Темп. нар. возд.","Макс.","°CWB","18"]
["","","","Мин.","°CWB","-15"]
["Подсоединение труб","Перепад уровней","IU - IU","Макс.","м","7.5"]
["","","IU - OU","Макс.","м","15"]
["","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)"]
["","Общая длина трубопроводов","Система","Фактическая","м","60"]
["Компрессор","Type","","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","936","936"]
["","","","Глубина","мм","300","300"]
["","","","Высота","мм","735","735"]
["Масса","Блок","","","кг","58","58"]
["Power supply","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","230","230"]
["Примечания","","","","","(1) - Охлаждение: темп. в помещении: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB; эквивалентная длина трубопроводов: 5 м","(1) - Охлаждение: темп. в помещении: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB; эквивалентная длина трубопроводов: 5 м"]
["","","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м"]
["","","","","","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы"]
["Подсоединение труб","Перепад уровней","IU - IU","Макс.","м","","7.5"]
["","","IU - OU","Макс.","м","","15"]
["","Дополнительная заправка хладагента","","","кг/м","","0,02 (для длины труб свыше 30 м)"]
["","Общая длина трубопроводов","Система","Фактическая","м","","60"]
["Компрессор","Type","","","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","735"]
["","","","Ширина","мм","","","936"]
["","","","Глубина","мм","","","300"]
["Масса","Блок","","","кг","","","58"]
["Компрессор","Type","","","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","","-10"]
["","","","Макс.","°C сух.т.","","","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","","-15"]
["","","","Макс.","°CWB","","","15.5"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","","","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","","","49"]
["Хладагент","Тип","","","","","","R-410A"]
["","Заправка","","","кг","","","2.6"]
["","Заправка","","","tCO2Eq","","","5.4"]
["","ПГП","","","","","","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","","25"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","","","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","","","15"]
["","","IU - IU","Макс.","м","","","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","","","60"]
["Стандартные аксессуары","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Электропитание","Фаза","","","","","","1~"]
["","Частота","","","Гц","","","50"]
["","Напряжение","","","V","","","230"]