{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Уровень звукового давления","Hагрев","","Ном.","дБ(A)","","49.0"]
["","Охлаждение","","Ном.","дБ(A)","","49.0"]
["Стандартные аксессуары","Сливная пробка","","","","","1"]
["","Инструкции по установке","","","","","1"]
["","Табличка с данными о заправке хладагентом","","","","","1"]
["","Этикетки о фторированных парниковых газах на нескольких языках","","","","","1"]
["","Общие меры предосторожности","","","","","1"]
["Хладагент","Charge","","","TCO2Eq","","0.52"]
["","ПГП","","","","","675"]
["","Charge","","","кг","","0.76"]
["","Тип","","","","","R-32"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Макс.","°CDB","","50 (4), 46 (5)"]
["","","","Мин.","°CDB","","-10"]
["Подсоединение труб","Перепад уровней","IU - OU","Макс.","м","","15"]
["","Дополнительная заправка хладагента","","","кг/м","","0,02 (для длины труб свыше 10 м)"]
["Компрессор","Type","","","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","","840"]
["","","","Глубина","мм","","350"]
["","","","Высота","мм","","552"]
["Масса","Блок","","","кг","","32"]
["Power supply","Phase","","","","","1~"]
["","Частота","","","Гц","","50"]
["","Напряжение","","","V","","220-240"]
["Примечания","","","","","(1) - Возможно только в сочетании с ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Содержит фторированные парниковые газы"]
["","","","","","(2) - Возможно только в сочетании с ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","(3) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","(4) - Возможно только в сочетании с ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Возможно только в сочетании с ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","552"]
["","","","Ширина","мм","840"]
["","","","Глубина","мм","350"]
["Масса","Блок","","","кг","32"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10"]
["","","","Макс.","°CDB","50 (4), 46 (5)"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","46.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","47.0"]
["Хладагент","Заправка","","","кг","0.76"]
["","Заправка","","","tCO2Eq","0.52"]
["","ПГП","","","","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Электропитание","Частота","","","Гц","50"]