{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N / ARXM-R"]
[]
[]
[]
[]
["","","","","ATXM35N2V1B / ARXM35R5V1B"]
["Наружный блок","","","","ARXM35R5V1B"]
["Холодопроизводительность","Мин.","","кВт","1.40"]
["","Ном.","","кВт","3.40"]
["","Макс.","","кВт","4.00"]
["Теплопроизводительность","Мин.","","кВт","1.40"]
["","Ном.","","кВт","4.00"]
["","Макс.","","кВт","5.20"]
["Номинальная эффективность","EER","","","4.09"]
["","COP","","","4.04"]
["","Годовое потребление энергии","","кВтч","416"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A+++"]
["","Производительность","Pрасч.","кВт","3.40"]
["","SEER","","","8.55"]
["","Годовое потребление энергии","","кВтч/г","139"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+++"]
["","Производительность","Pрасч.","кВт","2.50"]
["","SCOP/A","","","5.10"]
["","Pdh Теплопроизводительность при -10°","","кВт","2.35"]
["","Годовое потребление энергии","","кВтч/г","687"]
["Диапазон энергоэффективности","","","","A+++ ~ D"]