{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":6,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3"]
[]
[]
[]
[]
["","","","","","ATXP25K3V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.019"]
["","Hагрев","","Ном.","кВт","0.02"]
["Корпус","Цвет","","","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","286"]
["","","","Ширина","мм","770"]
["","","","Глубина","мм","225"]
["Масса","Блок","","","кг","9"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","10.1"]
["","","","Средн.","м³/мин","8.1"]
["","","","Низк.","м³/мин","6.1"]
["","","","Тихая работа","м³/мин","4.4"]
["","","Hагрев","Выс.","м³/мин","10.3"]
["","","Нагрев","Средн.","м³/мин","8.6"]
["","","Hагрев","Низк.","м³/мин","6.7"]
["","","","Тихая работа","м³/мин","5.3"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","55"]
["","Отопление","","","дБ(A)","55"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","40"]
["","","","Средн.","дБ(A)","33"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","26"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","20"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","40"]
["","Нагрев","","Средн.","дБ(A)","34"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","28"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","21"]
["Подсоединение труб","Жидкость","","НД","мм","6.35"]
["","Газ","","НД","мм","9.5"]
["","Дренаж","","","","18"]
["Системы управления","Infrared remote control","","","","ARC480A11"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]