{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Уровень звукового давления","Hагрев","Выс.","дБA","45","49"]
["","","Ном.","дБA","42","45"]
["","","Средн.","дБA","42","45"]
["","","Низк.","дБA","40","41"]
["","Охлаждение","Средн.","дБA","42","45"]
["","","Низк.","дБA","40","41"]
["","","Выс.","дБA","45","49"]
["","","Ном.","дБA","42","45"]
["Холодопроизводительность","Общая производительность","Ном.","кВт","0.051","0.061"]
["Подсоединение труб","Жидкость","НД","mm","9.52","9.52"]
["","Газ","НД","mm","15.9","15.9"]
["","Drain","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Sound power level","Охлаждение","","дБA","61","65"]
["","Отопление","","дБA","61","65"]
["Размеры","Блок","Ширина","mm","1,050","1,200"]
["","","Глубина","mm","238","240"]
["","","Высота","mm","290","340"]
["Корпус","Материал","","","Полимер","Полимер"]
["","Цвет","","","Яркий белый","Яркий белый"]
["Масса","Блок","","кг","13","17"]
["Теплопроизводительность","Общая производительность","Ном.","кВт","0.068","0.061"]
["Power supply","Phase","","","1~","1~"]
["","Частота","","Гц","50","50"]
["","Напряжение","","V","220-240","220-240"]