{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CAVEB / RZQG71L8Y1B","FHQ71CAVEB / RZQG71L8Y1B","FHQ100CAVEB / RZQG100L8Y1B","FHQ140CAVEB / RZQG100L8Y1B","FHQ125CAVEB / RZQG125L8Y1B","FHQ140CAVEB / RZQG125L8Y1B","FHQ140CAVEB / RZQG140L7Y1B","FHQ71CAVEB / FHQ71CAVEB / RZQG125L8Y1B (Archived)"]
["Холодопроизводительность","Ном.","","кВт","","6.8","9.5","","12.0","","13.4"]
["Охлаждение помещений","SEER","","","6.95","6.95","6.11","6.11","6.01","6.01"]
["","Годовое потребление энергии","","кВтч/г","343","343","545","545","699","699"]
["","Производительность","Pрасч.","кВт","6.80","6.8","9.5","9.50","12","12.00"]
["","Класс энергоэффективности","","","A++","A++","A++","A++","A+","A+"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","7.60","7.6","11.3","11.30","14.13","14.13"]
["","SCOP/A","","","4.32","4.32","4.61","4.61","4.23","4.23"]
["","Класс энергоэффективности","","","A+","A+","A++","A++","A+","A+"]
["","Годовое потребление энергии","","кВтч/г","2,463","2,463","3,432","3,432","4,677","4,677"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","","890","1,245","","1,790"]
["","EER","","","","3.82","3.81","","3.35","","3.31"]
["","COP","","","","4.13","4.15","","3.89","","3.63"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","A","A","","A"]
["","","Нагрев","","","A","A","","A"]
["Теплопроизводительность","Ном.","","кВт","","7.5","10.8","","13.5","","15.5"]
["Примечания","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["Наружный блок","","","","","","","","","","","RZQG125L8Y1"]
["Охлаждение помещений","Класс энергоэффективности","","","","","","","","","","B"]
["","Производительность","Pрасч.","кВт","","","","","","","","12.00"]
["","SEER","","","","","","","","","","5.10"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","824"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","","","","","","","","A"]
["","Производительность","Pрасч.","кВт","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","3.80"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","4683"]