{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.03","0.030","0.030"]
["","Hагрев","","Ном.","кВт","0.04","0.040","0.040"]
["Корпус","Цвет","","","","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","198","198","198"]
["","","","Ширина","мм","770","770","770"]
["","","","Глубина","мм","283","283","283"]
["Масса","Блок","","","кг","7","7.00","7.00"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.1","9.2","9.3"]
["","","","Средн.","м³/мин","7.4","7.6","7.7"]
["","","","Низк.","м³/мин","5.9","6.0","6.1"]
["","","","Тихая работа","м³/мин","4.7","4.8","4.9"]
["","","Hагрев","Выс.","м³/мин","9.4","9.7","10.1"]
["","","Нагрев","Средн.","м³/мин","7.8","8.0","8.4"]
["","","Hагрев","Низк.","м³/мин","6.3","6.3","6.7"]
["","","","Тихая работа","м³/мин","5.5","5.5","5.7"]
["Уровень звуковой мощности","Охлаждение","","","дБA","55","55","58"]
["","Отопление","","","дБA","55","55","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","39","40","41"]
["","","","Средн.","дБA","33","33","34"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","26","27"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","22","22","23"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39","40","41"]
["","Нагрев","","Средн.","дБA","34","34","35"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","28","28","29"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","25","25","26"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.50","9.50"]
["","Дренаж","","","","18","18","18"]
["Системы управления","Infrared remote control","","","","ARC433A87","ARC433A87","ARC433A87"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]