{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BB / RXJ20M5V1B9","FTXJ25A2V1BB / RXJ25M5V1B9","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ35A2V1BB / RXJ35M5V1B9"]
["Холодопроизводительность","Ном.","","кВт","","","3.50"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","","","428"]
["","EER","","","","","4.09"]
["","COP","","","","","4.04"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","A"]
["","","Нагрев","","","","A"]
["Теплопроизводительность","Ном.","","кВт","","","4.00"]
["Примечания","","","","","","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","(3) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","","(4) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["Наружный блок","","","","RXJ20M5V1B9","RXJ25M5V1B9","","RXJ35M5V1B9"]
["Холодопроизводительность","Ном.","","кВт","2.30","2.40","","3.50"]
["Теплопроизводительность","Ном.","","кВт","2.50","3.20","","4.00"]
["Номинальная эффективность","EER","","","4.64","4.73","","4.09"]
["","COP","","","5.00","4.57","","4.04"]
["","Годовое потребление энергии","","кВтч","248","254","","428"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","","A"]
["","","Нагрев","","A","A","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A+++","A+++","","A++"]
["","Производительность","Pрасч.","кВт","2.30","2.40","","3.50"]
["","SEER","","","8.73","8.64","","7.19"]
["","Годовое потребление энергии","","кВтч/г","92","97","","170"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A++","A++","","A++"]
["","Производительность","Pрасч.","кВт","2.10","2.70","","3.00"]
["","SCOP/A","","","4.61","4.60","","4.60"]
["","Pdh Теплопроизводительность при -10°","","кВт","1.80","2.18","","2.61"]
["","Годовое потребление энергии","","кВтч/г","638","822","","913"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]