{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AW"]
[]
[]
[]
[]
["","","","","","FTXJ20A2V1BW","FTXJ25A2V1BW","FTXJ35A2V1BW","FTXJ42A2V1BW","FTXJ50A2V1BW"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.02","0.022","0.024","0.028","0.031"]
["","Hагрев","","Ном.","кВт","0.021","0.022","0.024","0.036","0.039"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","305","305","305","305","305"]
["","","","Ширина","мм","900","900","900","900","900"]
["","","","Глубина","мм","212","212","212","212","212"]
["Масса","Блок","","","kg","12","12","12","12","12"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","11","11.4","11.8","13","13.5"]
["","","","Средн.","м³/мин","8.4","8.6","8.6","9.5","10.4"]
["","","","Низк.","м³/мин","6","6","6","7.2","7.6"]
["","","","Тихая работа","м³/мин","4.6","4.6","4.6","4.6","5.2"]
["","","Hагрев","Выс.","м³/мин","11.1","11.3","11.7","14.4","15.0"]
["","","Нагрев","Средн.","м³/мин","8.7","9","9","10.5","11.1"]
["","","Hагрев","Низк.","м³/мин","6.4","6.4","6.4","7.7","8.2"]
["","","","Тихая работа","м³/мин","4.6","4.6","4.6","5.2","5.7"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","57","57","60","60","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","39","40","41","45","46"]
["","","","Средн.","дБ(A)","32","33","33","37","39"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","25","25","25","29","31"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","19","19","19","21","24"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","39","40","41","45","46"]
["","Нагрев","","Средн.","дБ(A)","32","33","33","37","42"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","25","25","25","29","33"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","19","19","19","21","24"]
["Хладагент","ПГП","","","","675","675","675","675","675"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5","12.7","12.7"]
["","Дренаж","","","","18","18","18","18","18"]
["Системы управления","Infrared remote control","","","","ARC488A1W","ARC488A1W","ARC488A1W","ARC488A1W","ARC488A1W"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240","220-240"]