{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":24,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-A / 3MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM20A5V1B / FTXM20A5V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A5V1B / FTXM20A5V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM20A5V1B / FTXM25A2V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A5V1B / FTXM25A2V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM20A5V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A5V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM25A2V1B / FTXM25A2V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM25A2V1B / FTXM25A2V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM25A2V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM25A2V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM25A5V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM25A5V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM20A2V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM20A2V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM20A5V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM20A5V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM25A2V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM25A2V1B / FTXM35A5V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM25A5V1B / FTXM35A2V1B / 3MXM52A2V1B9","FTXM20A2V1B / FTXM25A5V1B / FTXM35A5V1B / 3MXM52A2V1B9"]
["Холодопроизводительность","Ном.","","кВт","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2"]
["Теплопроизводительность","Ном.","","кВт","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8","6.8"]
["Номинальная эффективность","EER","","","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76","4.76"]
["","COP","","","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88","4.88"]
["","Годовое потребление энергии","","кВтч","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546","546"]
["","Директива о маркировке классов энергоэффективности","Нагрев","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Производительность","Pрасч.","кВт","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2","5.2"]
["","SEER","","","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51","8.51"]
["","Годовое потребление энергии","","кВтч/г","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214","214"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Производительность","Pрасч.","кВт","5","5","5","5","5","5","5","5","5","5","5","5","5","5","5","5","5","5","5","5"]
["","SCOP/A","","","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1","5.1"]
["","Pdh Теплопроизводительность при -10°","","кВт","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1","4.1"]
["","Годовое потребление энергии","","кВтч/г","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373","1373"]