{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","40","","","","","","45"]
["","","","Тихая работа","дБ(A)","19","","","","","","22"]
["","","","Низк.","дБ(A)","27","","","","","","33"]
["","Охлаждение","","Тихая работа","дБ(A)","19","","","","","","21"]
["","","","Низк.","дБ(A)","24","","","","","","33"]
["","","","Выс.","дБ(A)","40","","","","","","45"]
["","","","Ном.","дБ(A)","34","","","","","","39"]
["","Охлаждение","","Ном.","дБ(A)","32","","","","","","39"]
["Стандартные аксессуары","Инструкции по установке","","","","1","","","","","","1"]
["","Руководство по эксплуатации","","","","1","","","","","","1"]
["","Беспроводной пульт дистанционного управления","","","","1","","","","","","1"]
["","Батареи","","","","2","","","","","","2"]
["","Держатель пульта дистанционного управления","","","","1","","","","","","1"]
["","Монтажная пластина","","","","1","","","","","","1"]
["","Крепежные винты внутреннего блока","","","","2","","","","","","2"]
["","Титано-апатитовый фотокаталитический фильтр","","","","2","","","","","","2"]
["Системы управления","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","","","","","","6.35"]
["","Газ","","НД","мм","9.5","","","","","","9.5"]
["","Дренаж","","","","18","","","","","","18"]
["Power input","Охлаждение","","Ном.","кВт","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Hагрев","","Ном.","кВт","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Охлаждение","","","дБ(A)","58","","","","","","59"]
["","Отопление","","","дБ(A)","58","","","","","","59"]
["Размеры","Блок","","Ширина","мм","780","","","","","","900"]
["","","","Глубина","мм","215","","","","","","215"]
["","","","Высота","мм","289","","","","","","298"]
["Корпус","Цвет","","","","Белый","","","","","","Белый"]
["Масса","Блок","","","kg","8","","","","","","11"]
["Power supply","Фаза","","","","1~","","","","","","1~"]
["","Частота","","","Гц","50","","","","","","50"]
["","Наименование","","","","V1","","","","","","V1"]
["","Напряжение","","","В","220-240","","","","","","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - При подсоединении к наружному блоку многоблочной системы, см. технические характеристики подсоединяемого наружного блока.","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 220 В","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 230 В","(3) - 240В","(3) - 240В","(3) - 240В"]
["Входная мощность","Охлаждение","","Ном.","кВт","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Hагрев","","Ном.","кВт","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Корпус","Цвет","","","","","Белый","Белый","Белый","Белый","Белый","","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","215","289","215","298","215","","215","298","215"]
["","","","Ширина","мм","","780","780","780","900","900","","900","900","900"]
["","","","Глубина","мм","","289","215","289","215","298","","298","215","298"]
["Масса","Блок","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Средн.","м³/мин","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Низк.","м³/мин","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Тихая работа","м³/мин","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Hагрев","Выс.","м³/мин","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","Нагрев","Средн.","м³/мин","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Hагрев","Низк.","м³/мин","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Тихая работа","м³/мин","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","","58","58","58","59","59","","59","60","60"]
["","Отопление","","","дБ(A)","","58","58","58","59","59","","59","60","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","40","41","41","45","45","","45","46","46"]
["","","","Средн.","дБ(A)","","32","33","33","","37","","39","","40"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","","24","25","25","29","29","","33","34","34"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","","19","19","19","19","19","","21","23","23"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","40","41","41","45","45","","45","47","47"]
["","Нагрев","","Средн.","дБ(A)","","34","34","34","","39","","39","","40"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","","27","27","27","29","29","","33","34","34"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","","19","19","19","19","19","","22","24","24"]
["Подсоединение труб","Жидкость","","НД","мм","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Газ","","НД","мм","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Дренаж","","","","","18","18","18","18","18","","18","18","18"]
["Системы управления","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Стандартные аксессуары","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Электропитание","Наименование","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Фаза","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Частота","","","Гц","","50","50","50","50","50","","50","50","50"]
["","Напряжение","","","В","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Вентилятор","Расход воздуха","Охлаждение","Ном.","м³/мин","","","9.1","","11.2","","","","11.9"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","","","33","","37","","","","40"]
["Вентилятор","Расход воздуха","Hагрев","Ном.","м³/мин","","","8.0","","9.3","","","","10.8"]
["Уровень звукового давления","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","","","34","","39","","","","40"]
["Системы управления","Инфракрасный пульт ДУ","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Стандартные аксессуары","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Примечания","","","","","","","","","","","(4) - 240В"]