{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L8Y1B","FVQ100CVEB / RZQG71L8Y1B","FVQ140CVEB / RZQG100L8Y1B","FVQ125CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG140L7Y1B"]
["Холодопроизводительность","Ном.","","кВт","6.8","","","12.0","","13.4"]
["Охлаждение помещений","SEER","","","6.23","6.31","5.61","5.61","5.61"]
["","Годовое потребление энергии","","кВтч/г","383","378","593","748.663","749"]
["","Производительность","Pрасч.","кВт","6.80","6.80","9.50","12.00","12.00"]
["","Класс энергоэффективности","","","A++","A++","A+","A+","A+"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","6.33","6.33","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","3.87","3.87"]
["","Класс энергоэффективности","","","A+","A+","A+","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,189","2,189","3,767","4,087.855","4,088"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","1,010","","","1,870","","2,085"]
["","EER","","","3.37","","","3.21","","3.21"]
["","COP","","","3.64","","","3.70","","3.61"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","","","A"]
["","","Нагрев","","A","","","A"]
["Теплопроизводительность","Ном.","","кВт","7.5","","","13.5","","15.5"]
["Примечания","","","","(1) - Годовое потребление энергии соответствует Европейской директиве о маркировке 2002/31/EC","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - SEER и SCOP соответствуют EN 14825","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]