{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Руководство по эксплуатации","","","","1"]
["","Соединительные трубопроводы","","","","1"]
["","Ярлык хладагента для нормы по F-газам","","","","1"]
["","Табличка с данными о заправке хладагентом","","","","1"]
["","Этикетки о фторированных парниковых газах на нескольких языках","","","","1"]
["Масса","Блок","","","kg","370"]
["Хладагент","Charge","","","TCO2Eq","24.0"]
["","ПГП","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Тип","","","","R-410A"]
["Мотор вентилятора","Мощность","","","Вт","750"]
["","Привод","","","","Прямая передача"]
["Теплообменник","Тип","","","","Теплообменник с поперечным соединением оребрения"]
["Размеры","Блок","","Ширина","мм","1,240"]
["","","","Глубина","мм","765"]
["","","","Высота","мм","1,680"]
["Корпус","Цвет","","","","Слоновая кость_"]
["Вентилятор","Тип","","","","Осевой вентилятор"]
["","Расход воздуха","Охлаждение","Ном.","м³/мин","230"]
["","Кол-во","","","","2"]
["Power supply","Фаза","","","","3~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","В","380-415"]
["Примечания","","","","","(1) - Приоритетный режим при охлаждении: темп. в помещении: 27°CDB, 19°CWB; темп. наружного возд. 32°CDB; длина трубопровода: 7,5 м; перепад уровня: 0 м"]
["","","","","","(2) - Приоритетный режим при охлаждении: Температура испарения -10°C; темп. наружного возд. 32°CDB; Перегрев на всасывании: 10°C"]
["","","","","","(3) - Режим 100% рекуперации теплоты: темп. в помещении: 20°CDB; темп. наружного возд. 7°CDB, 6°CWB; нагрузка при технологическом охлаждении 18 кВт; длина трубопровода: 7,5 м; перепад уровня: 0 м"]
["","","","","","(4) - температура насыщения, эквивалентная давлению всасывания (сторона охлаждения): -10°C (в охлажденном состоянии); производительность при подсоед. для внутреннего кондиционера: 10 л.с., когда рекуперация теплоты равна 100%"]
["","","","","","(5) - Компрессор 1"]
["","","","","","(6) - Компрессор 2"]
["","","","","","(7) - Компрессор 3"]
["","","","","","(8) - Заводская заправка блока"]
["","","","","","(9) - Устанавливать маслоуловитель с интервалом 5 м от наружного блока"]
["","","","","","(10) - Более подробная информация приведена на чертеже рабочего диапазона"]
["","","","","","(11) - Более подробная информация о стандартных принадлежностях приведена в руководстве по монтажу/эксплуатации"]
["","","","","","(12) - Содержит фторированные парниковые газы"]