{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Тип","","","","","Увлажняющий воздухоочиститель"]
["Применение","","","","","Напольный тип"]
["Корпус","Цвет","","","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","mm","700"]
["","","","Ширина","mm","270"]
["","","","Глубина","mm","270"]
["Масса","Блок","","","кг","9.5"]
["Обслуживаемая площадь","m²","","","","41 (1), 82 (2)"]
["CADR","м³/ч","","","","320"]
["Режим очистки воздуха","Входная мощность","","Turbo","кВт","0.056"]
["","","","M","кВт","0.017"]
["","","","L","кВт","0.010"]
["","","","Бесшумный","кВт","0.007"]
["Режим увлажнения","Входная мощность","","Turbo","кВт","0.058"]
["","","","M","кВт","0.019"]
["","","","L","кВт","0.014"]
["","","","Бесшумный","кВт","0.011"]
["","Емкость водяного бака","","","л","2.7"]
["Уровень звукового давления","Режим очистки воздуха","","Turbo","дБA","53.0"]
["","","","Средн.","дБA","39.0"]
["","","","Низк.","дБA","29.0"]
["","","","Бесшумный","дБA","19.0"]
["","Режим увлажнения","","Turbo","дБA","53.0"]
["","","","Средн.","дБA","39.0"]
["","","","Низк.","дБA","33.0"]
["","","","Бесшумный","дБA","25.0"]
["Вентилятор","Расход воздуха","Режим очистки воздуха","Turbo","м³/ч","330"]
["","","","Средний уровень","м³/ч","192"]
["","","","Низк.","м³/ч","120"]
["","","","Бесшумный","м³/ч","54"]
["","","Режим увлажнения","Turbo","м³/ч","330"]
["","","","Средний уровень","м³/ч","192"]
["","","","Низк.","м³/ч","144"]
["","","","Бесшумный","м³/ч","102"]
["Способ пылеудаления","","","","","Электростатический HEPA-фильтр"]
["Способ дезодорирования","","","","","Стримерный разряд + дезодорирующий катализатор"]
["Стандартные аксессуары","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Шнур питания","Шнур питания","","","","1.8"]
["Электропитание","Фаза","","","","1~"]
["","Электропитание-=-Частота","","Частота","","50/60"]
["","Электропитание-=-Напряжение","","Напряжение","","220-240/220-230"]
["Рабочий ток","Режим очистки воздуха","Рабочий ток-=-Режим очистки воздуха-=-Turbo","Turbo","","0.50"]
["","","Рабочий ток-=-Режим очистки воздуха-=-Средний уровень","Средний уровень","","0.19"]
["","","Рабочий ток-=-Режим очистки воздуха-=-Низк.","Низк.","","0.12"]
["","","Рабочий ток-=-Режим очистки воздуха-=-Бесшумный","Бесшумный","","0.09"]
["","Режим увлажнения","Рабочий ток-=-Режим увлажнения-=-Turbo","Turbo","","0.50"]
["","","Рабочий ток-=-Режим увлажнения-=-Средний уровень","Средний уровень","","0.20"]
["","","Рабочий ток-=-Режим увлажнения-=-Низк.","Низк.","","0.15"]
["","","Рабочий ток-=-Режим увлажнения-=-Бесшумный","Бесшумный","","0.13"]
["Примечания","","","","","(1) - Обслуживаемая площадь помещения подходит для работы блока при максимальной скорости вентилятора (HH). Обслуживаемая площадь помещения — это часть, в которой может быть удалено определенное количество частиц пыли за 30 минут. (JEM 1467)"]
["","","","","","(2) - Преобразовано в стандарты NRCC на основе результатов испытаний в соответствии с JEM1467."]