{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Тип","","","","","Увлажняющий воздухоочиститель"]
["Применение","","","","","Напольный тип"]
["Корпус","Цвет","","","","Белый (N9. 0)"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","mm","600 (5)"]
["","","","Ширина","mm","395"]
["","","","Глубина","mm","287"]
["Масса","Блок","","","кг","12.5"]
["Обслуживаемая площадь","m²","","","","48 (1), 96 (2)"]
["CADR","м³/ч","","","","375"]
["Режим очистки воздуха","Входная мощность","","Turbo","кВт","0.066"]
["","","","M","кВт","0.016"]
["","","","L","кВт","0.01"]
["","","","Бесшумный","кВт","0.008"]
["Режим увлажнения","Входная мощность","","Turbo","кВт","0.068"]
["","","","M","кВт","0.018"]
["","","","L","кВт","0.012"]
["","","","Бесшумный","кВт","0.011"]
["","Емкость водяного бака","","","л","3.6"]
["Уровень звукового давления","Режим очистки воздуха","","Turbo","дБA","54"]
["","","","Средн.","дБA","37"]
["","","","Низк.","дБA","27"]
["","","","Бесшумный","дБA","18"]
["","Режим увлажнения","","Turbo","дБA","54"]
["","","","Средн.","дБA","37"]
["","","","Низк.","дБA","27"]
["","","","Бесшумный","дБA","23"]
["Вентилятор","Расход воздуха","Режим очистки воздуха","Turbo","м³/ч","420"]
["","","","Средний уровень","м³/ч","210"]
["","","","Низк.","м³/ч","132"]
["","","","Бесшумный","м³/ч","60"]
["","","Режим увлажнения","Turbo","м³/ч","420"]
["","","","Средний уровень","м³/ч","210"]
["","","","Низк.","м³/ч","132"]
["","","","Бесшумный","м³/ч","102"]
["Способ пылеудаления","","","","","Электростатический HEPA-фильтр"]
["Способ дезодорирования","","","","","Стримерный разряд + дезодорирующий катализатор"]
["Стандартные аксессуары","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Шнур питания","м","","","","2"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50/60"]
["","Напряжение","","","V","220-240/220-230"]
["Примечания","","","","","(1) - Обслуживаемая площадь соответствует работе блока при максимальной скорости вентилятора (HH). Обслуживаемая площадь помещения — это пространство, из которого может быть удалено определенное количество частиц пыли за 30 минут."]
["","","","","","(2) - Преобразовано в стандарты NRCC на основе результатов испытаний в соответствии с JEM1467."]
["","","","","","(3) - Уровни звукового давления в процессе работы представляют собой средние значения, измеряемые на расстоянии 1 м от передней, левой, правой и верхней стороны блока. (Эти значения равны значению в безэховой камере)"]