{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXB-B"]
[]
[]
[]
[]
["","","","","","RXB25B5V1","RXB25B6V1","RXB25B6V19","RXB35B5V1","RXB35B6V1","RXB35B6V19","RXB50BV1B","RXB60BV1B"]
["Уровень звукового давления","Hагрев","","Ном.","дБA","","","","","","","51","51"]
["","Охлаждение","","Ном.","дБA","","","","","","","51","51"]
["Хладагент","Charge","","","TCO2Eq","","","","","","","3","3"]
["","ПГП","","","","","","","","","","2,087.5","2,087.5"]
["","Charge","","","кг","","","","","","","1.45","1.45"]
["","Тип","","","","","","","","","","R-410A","R-410A"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Макс.","°C сух.т.","","","","","","","46","46"]
["","","","Мин.","°C сух.т.","","","","","","","-10","-10"]
["","Hагрев","Темп. нар. возд.","Макс.","°CWB","","","","","","","18","18"]
["","","","Мин.","°CWB","","","","","","","-15","-15"]
["Компрессор","Тип","","","","","","","","","","Герметичный ротационный","Герметичный ротационный"]
["Размеры","Блок","","Ширина","мм","","","","","","","855","855"]
["","","","Глубина","мм","","","","","","","328","328"]
["","","","Высота","мм","","","","","","","753","753"]
["Масса","Блок","","","кг","","","","","","","44","44"]
["Power supply","Фаза","","","","","","","","","","1~","1~"]
["","Частота","","","Гц","","","","","","","50","50"]
["","Напряжение","","","В","","","","","","","220-240","220-240"]
["Примечания","","","","","","","","","","","(1) - Все блоки протестированы и удовлетворяют требованиям ISO 5151 (бесканальные блоки) или ISO 13253 (канальные блоки).","(1) - Все блоки протестированы и удовлетворяют требованиям ISO 5151 (бесканальные блоки) или ISO 13253 (канальные блоки)."]
["","","","","","","","","","","","(2) - Все технические характеристики могут быть изменены изготовителем без предварительного уведомления.","(2) - Все технические характеристики могут быть изменены изготовителем без предварительного уведомления."]
["","","","","","","","","","","","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","550","550","550","550"]
["","","","Ширина","мм","658","658","658","658","658","658"]
["","","","Глубина","мм","275","275","275","275","275","275"]
["Масса","Блок","","","кг","27","26","26","29","28","28"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","46","46","46","48","48","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","47","47","47","48","48","48"]
["Хладагент","Тип","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Заправка","","","кг","0.74","0.74","0.74","1.00","1.00","1.00"]
["","Заправка","","","tCO2Eq","1.5","1.5","1.5","2.1","2.1","2.1"]
["","ПГП","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","15","15","15","15","15","15"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","12","12","12","12","12","12"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240","220-240","220-240"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","-10","-10","","-10","-10"]
["","","","Макс.","°C сух.т.","","46","46","","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","-15","-15","","-15","-15"]
["","","","Макс.","°CWB","","18","18","","18","18"]