{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-MB"]
[]
[]
[]
[]
["","","","","","RXN25MV1B","RXN35MV1B","RXN50MV1B","RXN60MV1B"]
["Уровень звукового давления","Hагрев","","Ном.","дБ(A)","","","","51"]
["","Охлаждение","","Ном.","дБ(A)","","","","51"]
["Хладагент","Charge","","","TCO2Eq","","","","3"]
["","ПГП","","","","","","","2,087.5"]
["","Charge","","","кг","","","","1.45"]
["","Тип","","","","","","","R-410A"]
["Compressor","Тип","","","","","","","Герметичный ротационный"]
["Размеры","Блок","","Ширина","мм","","","","855"]
["","","","Глубина","мм","","","","328"]
["","","","Высота","мм","","","","753"]
["Масса","Блок","","","кг","","","","44"]
["Power supply","Фаза","","","","","","","1~"]
["","Частота","","","Гц","","","","50"]
["","Напряжение","","","V","","","","220-240"]
["Примечания","","","","","","","","(1) - Все технические характеристики могут быть изменены изготовителем без предварительного уведомления."]
["","","","","","","","","(2) - Содержит фторированные парниковые газы"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","753"]
["","","","Ширина","мм","658","658","855"]
["","","","Глубина","мм","289","289","328"]
["Масса","Блок","","","кг","31","31","44"]
["Компрессор","Тип","","","","Герметичный ротационный","Герметичный ротационный","Герметичный ротационный"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","10","10","-10"]
["","","","Макс.","°C сух.т.","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15","-15"]
["","","","Макс.","°CWB","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","45","46","51"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","45","46","51"]
["Хладагент","Тип","","","","R-410A","R-410A","R-410A"]
["","Заправка","","","кг","1.00","1.00","1.45"]
["","Заправка","","","tCO2Eq","2.1","2.1","3"]
["","ПГП","","","","2087.5","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","30"]
["Электропитание","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]