{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","46.0"]
["","","Нагрев","Сверхнизкий","м³/мин","46.0"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","фт3/мин","1624"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","фт3/мин","1624"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","770"]
["","","","Ширина","мм","900"]
["","","","Глубина","мм","320"]
["Масса","Блок","","","кг","71"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","730"]
["","","Нагревание","Самый низкий","об/мин","730"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10"]
["","","","Макс.","°CDB","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15"]
["","","","Макс.","°CWB","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","52"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","52"]
["Хладагент","Тип","","","","R-410A"]
["","Заправка","","","кг","2.3"]
["","Заправка","","","tCO2Eq","4.8"]
["","ПГП","","","","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","20"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]
["Примечания","","","","","(1) - 220 В"]
["","","","","","(2) - 230 В"]
["","","","","","(3) - 240В"]