{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Размеры","Блок","","Высота","mm","870","870"]
["","","","Ширина","mm","1,100","1,100"]
["","","","Глубина","mm","460","460"]
["Масса","Unit","","","кг","117","117"]
["Компрессор","Тип","","","","Герметичный спиральный компрессор","Герметичный спиральный компрессор"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-20","-20"]
["","","","Макс.","°C сух.т.","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-20","-20"]
["","","","Макс.","°CWB","15","15"]
["Sound power level","Охлаждение","","","дБA","73","76"]
["","Отопление","","","дБA","76 (1)","79 (1)"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","53","57"]
["","Hагрев","","Ном.","дБA","60","63"]
["Хладагент","Тип","","","","R-32","R-32"]
["","Заправка","","","кг","5","5"]
["","ПГП","","","","675","675"]
["Подсоединение труб","Жидкость","","НД","mm","9.52","9.52"]
["","Газ","","НД","mm","22.2","22.2"]
["","Длина трубы","Макс.","НБ - ВБ","м","100","100"]
["","","Система","Без заправки","м","30","30"]
["","Дополнительная заправка хладагента","","","кг/м","См. инструкции по установке","См. инструкции по установке"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1"]
["","Общие меры предосторожности","","","","1","1"]
["","Хомуты","","","","2","2"]
["","Отклеиваемая информационная табличка об F-газах","","","","1","1"]
["","Соединительные трубопроводы","","","","6","6"]
["Power supply","Фаза","","","","3~","3~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","380-415","380-415"]
["Ток - 50 Гц","Макс. ток предохранителя (MFA)","","","A","20","20"]
["Примечания","","","","","(1) - Согласно ENER Lot 21","(1) - Согласно ENER Lot 21"]