{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Уровень звукового давления","Hагрев","Выс.","дБ(A)","36","37","37","38"]
["","","Ном.","дБ(A)","34","35","35","36"]
["","","Средн.","дБ(A)","31","32","33","34"]
["","Охлаждение","Средн.","дБ(A)","34","35","35","36"]
["","","Низк.","дБ(A)","31","32","33","34"]
["","","Выс.","дБ(A)","36","37","37","38"]
["Стандартные аксессуары","Теплоизолированная труба","","","2","2","2","2"]
["","Материал кабельного зажима","","","7","7","7","7"]
["","Хомут для шланга","","","1","1","1","1"]
["","Сливной шланг","","","1","1","1","1"]
["","Шайба","","","8","8","8","8"]
["","Уплотнительная подушка (большая)","","","1","1","1","1"]
["","Уплотнительная подушка (малая)","","","1","1","1","1"]
["","Полимерная втулка","","","1","1","1","1"]
["","Винты","","","2","2","2","2"]
["","Крепление проводки","","","2","2","2","2"]
["Системы управления","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Подсоединения труб","Жидкость","OD","мм","6.35","6.35","6.35","9.52"]
["","Газ","OD","мм","9.50","12.7","12.7","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20"]
["Уровень звуковой мощности","Cooling","","дБ(A)","53","54","54","55"]
["Размеры","Unit","Width","мм","960","960","1,270","1,270"]
["","","Depth","мм","690","690","690","690"]
["","","Высота","мм","235","235","235","235"]
["Корпус","Material","","","Полимер, листовой металл","Полимер, листовой металл","Полимер, листовой металл","Полимер, листовой металл"]
["","Цвет","","","Белый","Белый","Белый","Белый"]
["Вес","Блок","","кг","24.0","25.0","31.0","32.0"]
["Power supply","Фаза","","","1~","1~","1~","1~"]
["","Частота","","Гц","50","50","50","50"]
["","Напряжение","","V","220-240","220-240","220-240","220-240"]
["Примечания","","","","(1) - Электрические параметры см. в отдельных чертежах","(1) - Электрические параметры см. в отдельных чертежах","(1) - Электрические параметры см. в отдельных чертежах","(1) - Электрические параметры см. в отдельных чертежах"]